(footprint "SW_Push_1P1T_NO_6x6mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "tactile push button, 6x6mm e.g. PTS645xx series, height=9.5mm")
	(tags "tact sw push 6mm smd")
	(property "Reference" "REF**"
		(at 0 -4.05 0)
		(layer "F.SilkS")
		(uuid "988d92ba-58e9-481f-9771-61033aed70ee")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SW_Push_1P1T_NO_6x6mm"
		(at 0 4.15 0)
		(layer "F.Fab")
		(uuid "eeb86a43-f4c8-46f1-92a9-461c1a683322")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c9b37d53-5ef8-467f-bacc-2c5583b6edaa")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e9854b9f-a3d5-4375-933f-fd79e4dff803")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7f191908-a8bc-43ed-ac7f-16d84ce73177")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.23 -3.23)
		(end 3.23 -3.23)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0bca3493-1596-4de4-87d5-628f528d6902")
	)
	(fp_line
		(start -3.23 -3.2)
		(end -3.23 -3.23)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "972d95cc-c5ca-416c-960b-25d6a76511ee")
	)
	(fp_line
		(start -3.23 -1.25)
		(end -3.23 1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4b2b0a0d-065e-467a-b174-365fb6e12262")
	)
	(fp_line
		(start -3.23 3.23)
		(end -3.23 3.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1ae32315-7150-49da-8999-31c987c59159")
	)
	(fp_line
		(start -3.23 3.23)
		(end 3.23 3.23)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6ad38078-0ed7-486e-86b3-23edc420ead7")
	)
	(fp_line
		(start 3.23 -3.23)
		(end 3.23 -3.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "66790e40-eae1-4ba7-9d22-f44412671653")
	)
	(fp_line
		(start 3.23 -1.25)
		(end 3.23 1.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fd6f0938-efa6-4c8e-b90c-60ea623c907d")
	)
	(fp_line
		(start 3.23 3.23)
		(end 3.23 3.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d74bf154-13a4-4cb2-bbc3-09496a53d04e")
	)
	(fp_line
		(start -5.5 -3.25)
		(end -5.5 3.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0cf073d5-ff61-4ca5-af91-c5cb611a030a")
	)
	(fp_line
		(start -5.5 -3.25)
		(end 5.5 -3.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6f02bd5e-20de-46e5-8303-4285851cbbeb")
	)
	(fp_line
		(start -5.5 3.25)
		(end 5.5 3.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a9b65a2e-23a5-4659-a455-dfd81cfdc5f0")
	)
	(fp_line
		(start 5.5 3.25)
		(end 5.5 -3.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "60dc5c2e-b361-4761-9ab1-9da8539504d1")
	)
	(fp_line
		(start -3 -3)
		(end -3 3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3f775b1b-78e0-491b-af21-51a5d5c2c903")
	)
	(fp_line
		(start -3 3)
		(end 3 3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "73931746-b36c-48b3-bcaf-6c8852ba22a3")
	)
	(fp_line
		(start 3 -3)
		(end -3 -3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8771b831-4df7-46ee-af98-54929bcae505")
	)
	(fp_line
		(start 3 3)
		(end 3 -3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e26723d2-19d7-482b-9aaf-34413c5d5708")
	)
	(fp_circle
		(center 0 0)
		(end 1.75 -0.05)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "24e9c3c5-2d47-47bc-a3ac-90076b1ce0e4")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -4.05 0)
		(layer "F.Fab")
		(uuid "df8addff-29ed-4dd2-9b05-26c8b6df3635")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" smd rect
		(at 4.1 -2)
		(size 1.8 1.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "606ece18-3a9f-4d83-ac3f-76789dda7dd4")
	)
	(pad "" smd rect
		(at 4.1 2)
		(size 1.8 1.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "9b1d7e77-d06e-47b3-9f83-98d745df92c0")
	)
	(pad "1" smd rect
		(at -4.1125 -2)
		(size 1.775 1.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "ee106920-6ecf-45ee-94e7-a4dfd0c2fcb2")
	)
	(pad "2" smd rect
		(at -4.1 2)
		(size 1.8 1.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "0d00fb02-0ec0-4e67-ac65-6a49d54c1a5b")
	)
	(model "${KICAD8_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_PUSH_6mm_H9.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)