(footprint "HUSB238_Breakout"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
	(tags "Through hole pin header THT 1x07 2.54mm single row")
	(property "Reference" "REF**"
		(at 0 -2.33 0)
		(layer "F.SilkS")
		(uuid "8e76cb48-5cc8-4230-8363-3ba490a13d0a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "HUSB238_Breakout"
		(at 0 17.57 0)
		(layer "F.Fab")
		(uuid "803619fa-8158-4f02-b848-96250671bc9d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "05223517-c3a4-4374-b031-d698af543481")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d2faa408-619d-4aab-9b64-a089d08cd38d")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3cab57db-bc6c-4ae5-ae04-d8734313a6ae")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.33 -1.33)
		(end 0 -1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "882bed7b-2603-4740-ad95-cca87bd16440")
	)
	(fp_line
		(start -1.33 0)
		(end -1.33 -1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a244b5bf-6827-44ee-bea3-8ec454a0bd6a")
	)
	(fp_line
		(start -1.33 1.27)
		(end -1.33 16.57)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1a240e14-8489-4376-a58e-2ce70c038c45")
	)
	(fp_line
		(start -1.33 1.27)
		(end 1.33 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "16e7b6d7-acf2-4413-a154-ad3138e8df63")
	)
	(fp_line
		(start -1.33 16.57)
		(end 1.33 16.57)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "98d93693-9772-47dc-a941-6a605be1636a")
	)
	(fp_line
		(start 1.33 1.27)
		(end 1.33 16.57)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c1073b13-d57f-487f-87f9-4a51f6317bd5")
	)
	(fp_line
		(start -1.8 -1.8)
		(end -1.8 17.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3e4bdc11-4439-44e1-8645-dffdeee3095d")
	)
	(fp_line
		(start -1.8 17.05)
		(end 1.8 17.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "26f116e1-3769-48f2-8d32-68cce2dc8c2d")
	)
	(fp_line
		(start 1.8 -1.8)
		(end -1.8 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1217e94f-fdcb-4d0d-829d-ba425c0881f8")
	)
	(fp_line
		(start 1.8 17.05)
		(end 1.8 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "95d19fc7-a1c1-4dcb-9c2c-9ad3883dff59")
	)
	(fp_line
		(start -1.27 -0.635)
		(end -0.635 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "aaf13066-b90c-4e7b-a378-9ce47f78d930")
	)
	(fp_line
		(start -1.27 16.51)
		(end -1.27 -0.635)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c8ea947d-50f9-4f5c-92f4-623167229535")
	)
	(fp_line
		(start -0.635 -1.27)
		(end 1.27 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "af56e90b-a710-470f-8c5f-51e5612b784b")
	)
	(fp_line
		(start 1.27 -1.27)
		(end 1.27 16.51)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d35746b7-dcde-4cf3-8892-35673c90fa4a")
	)
	(fp_line
		(start 1.27 16.51)
		(end -1.27 16.51)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "bec6a7df-5703-4394-a2d9-934f3325a8dc")
	)
	(fp_text user "${REFERENCE}"
		(at 0 7.62 90)
		(layer "F.Fab")
		(uuid "2a60423e-2737-4a79-aacb-48e99c2086e6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c92221b7-e80e-4bcd-b8eb-7b86b4ce2e22")
	)
	(pad "2" thru_hole oval
		(at 0 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b5ca0c85-3307-4520-8c33-316547d43f87")
	)
	(pad "3" thru_hole oval
		(at 0 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3a83ddcd-c68d-461c-a70c-e73ce6b4cbc2")
	)
	(pad "4" thru_hole oval
		(at 0 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "65681c7e-de16-431d-ba61-aee7cadd5f28")
	)
	(pad "5" thru_hole oval
		(at 0 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "34044b43-d5fc-4a88-ac0e-1b4f2c624e08")
	)
	(pad "6" thru_hole oval
		(at 0 15.24)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ae856802-b50a-49c8-8fb4-184cc797903e")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)