(footprint "LED_1411_3528Metric_Pad1.42x2.65mm_HandSolder_copy"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "LED SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
	(tags "LED handsolder")
	(property "Reference" "REF**"
		(at 0 -2.28 0)
		(layer "F.SilkS")
		(uuid "09390470-db8b-4e93-870b-6fd878d5c088")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "LED_1210_3225Metric_Pad1.42x2.65mm_HandSolder"
		(at 0 2.28 0)
		(layer "F.Fab")
		(uuid "c0198d13-e751-4248-b58f-fff4a5fe8838")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e5f37d3e-8f75-4273-8bfa-58e3b142fdf1")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e29a6330-f104-493a-9d2d-6b1d55fc791a")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "936de873-0a8e-4f20-9fe4-d58d2759c4f1")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.46 -1.585)
		(end -2.46 1.585)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "49b883d0-f9cb-43da-902c-df905ca7644d")
	)
	(fp_line
		(start -2.46 1.585)
		(end 1.6 1.585)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8b2b637a-ae88-4a1c-b354-969b466e226c")
	)
	(fp_line
		(start 1.6 -1.585)
		(end -2.46 -1.585)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cded5001-e925-45cb-a3a7-204b32307a92")
	)
	(fp_line
		(start -2.45 -1.58)
		(end 3 -1.58)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "63887c82-c418-4c74-8e79-247c62386d82")
	)
	(fp_line
		(start -2.45 1.58)
		(end -2.45 -1.58)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "977abcd5-c373-44c8-bb16-07bdedb5cff3")
	)
	(fp_line
		(start 3 -1.58)
		(end 3 1.58)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f5ab7d83-db1b-46fe-b4d4-0be5431d3bae")
	)
	(fp_line
		(start 3 1.58)
		(end -2.45 1.58)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8966f193-eb7a-4f8a-a75c-68d6412c66a7")
	)
	(fp_line
		(start -1.6 -0.625)
		(end -1.6 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "489e1e5b-4389-4263-92ff-7fc17e4db6c4")
	)
	(fp_line
		(start -1.6 1.25)
		(end 2.75 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1c41c81d-679d-4f91-a17f-f1572ef82748")
	)
	(fp_line
		(start -0.975 -1.25)
		(end -1.6 -0.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "163494f4-93a5-491e-a20b-71d975c5ddf1")
	)
	(fp_line
		(start 2.75 -1.25)
		(end -0.975 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9da9702f-c8c5-45d8-90e1-b424b406d24b")
	)
	(fp_line
		(start 2.8025 1.25)
		(end 2.8025 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f43a5ff8-8b2e-4f1a-9297-853f5a689ce3")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "36aa2782-e8aa-4216-a852-1ff61d7d98f5")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.12)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1 0)
		(size 2.5 2.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.175439)
		(uuid "8dbd53a3-db73-4488-9a3e-f853471c5d44")
	)
	(pad "2" smd roundrect
		(at 2.09 0)
		(size 1.425 2.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.175439)
		(uuid "9695b557-0e14-4b87-a48a-e5aabb5edf1d")
	)
	(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1210_3225Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)